# CMSIS DSP Software Library: arm_offset_f32.c Source File

- Main Page
- Modules
- Data Structures
- Files
- Examples

- File List
- Globals

# arm_offset_f32.c

Go to the documentation of this file.

    00001 /* ----------------------------------------------------------------------
    00002 * Copyright (C) 2010 ARM Limited. All rights reserved.
    00003 *
    00004 * $Date:        15. July 2011
    00005 * $Revision:    V1.0.10
    00006 *
    00007 * Project:      CMSIS DSP Library
    00008 * Title:        arm_offset_f32.c
    00009 *
    00010 * Description:  Floating-point vector offset.
    00011 *
    00012 * Target Processor: Cortex-M4/Cortex-M3/Cortex-M0
    00013 *
    00014 * Version 1.0.10 2011/7/15
    00015 *    Big Endian support added and Merged M0 and M3/M4 Source code.
    00016 *
    00017 * Version 1.0.3 2010/11/29
    00018 *    Re-organized the CMSIS folders and updated documentation.
    00019 *
    00020 * Version 1.0.2 2010/11/11
    00021 *    Documentation updated.
    00022 *
    00023 * Version 1.0.1 2010/10/05
    00024 *    Production release and review comments incorporated.
    00025 *
    00026 * Version 1.0.0 2010/09/20
    00027 *    Production release and review comments incorporated.
    00028 *
    00029 * Version 0.0.7  2010/06/10
    00030 *    Misra-C changes done
    00031 * ---------------------------------------------------------------------------- */
    00032
    00033 #include "arm_math.h"
    00034
    00066 void arm_offset_f32(
    00067   float32_t * pSrc,
    00068   float32_t offset,
    00069   float32_t * pDst,
    00070   uint32_t blockSize)
    00071 {
    00072   uint32_t blkCnt;                               /* loop counter */
    00073
    00074 #ifndef ARM_MATH_CM0
    00075
    00076 /* Run the below code for Cortex-M4 and Cortex-M3 */
    00077
    00078   /*loop Unrolling */
    00079   blkCnt = blockSize >> 2u;
    00080
    00081   /* First part of the processing with loop unrolling.  Compute 4 outputs at a time.
    00082    ** a second loop below computes the remaining 1 to 3 samples. */
    00083   while(blkCnt > 0u)
    00084   {
    00085     /* C = A + offset */
    00086     /* Add offset and then store the results in the destination buffer. */
    00087     *pDst++ = (*pSrc++) + offset;
    00088     *pDst++ = (*pSrc++) + offset;
    00089     *pDst++ = (*pSrc++) + offset;
    00090     *pDst++ = (*pSrc++) + offset;
    00091
    00092     /* Decrement the loop counter */
    00093     blkCnt--;
    00094   }
    00095
    00096   /* If the blockSize is not a multiple of 4, compute any remaining output samples here.
    00097    ** No loop unrolling is used. */
    00098   blkCnt = blockSize % 0x4u;
    00099
    00100 #else
    00101
    00102   /* Run the below code for Cortex-M0 */
    00103
    00104   /* Initialize blkCnt with number of samples */
    00105   blkCnt = blockSize;
    00106
    00107 #endif /* #ifndef ARM_MATH_CM0 */
    00108
    00109   while(blkCnt > 0u)
    00110   {
    00111     /* C = A + offset */
    00112     /* Add offset and then store the result in the destination buffer. */
    00113     *pDst++ = (*pSrc++) + offset;
    00114
    00115     /* Decrement the loop counter */
    00116     blkCnt--;
    00117   }
    00118 }
    00119

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines